CHICHESTER BAR

Chichester Bar is periodically dredged to 1•5 metres below Chart Datum; shoaling to a minimum depth of 0.7 metres occurs between dredges and particularly after strong winds. Chichester Harbour Master should be consulted for the latest information. Dangerous seas may be encountered in strong onshore winds, especially during the ebb tide.


