AREA TO BE AVOIDED BETWEEN THE SMALLS AND GRASSHOLM

To avoid the risk of pollution due to stranding, vessels laden with oil, gas or 
noxious liquid substances, and all other vessels of more than 500 gt, should 
avoid this area.

