GENERAL INFORMATION FOR THE SOTE CANAL
Bridge opening:
Before entering the canal, call Sotenäs bridge on VHF ch 6 
or give following blasts 0,5 M from the bridge:

Northbound: 2 long and 1 short
Southbound: 2 long and 2 short

Bridgesignals:
F R	Bridge closed or unclear.
Fl R	Signal acknowledged, stand by.
F G	Bridge open, proceed.

Attention and reply signals:
Northbound: 1 long and 1 short
Southbound: 1 short and 1 long
Sailing is prohibited in the Sote canal.
Contact information, visit www.sjofartsverket.se