CABLE FERRY MALÖ STRÖMMAR
Vessels approaching the ferry route shall give one long blast
with signal horn.
RESTRICTED DEPTH ABOVE CABLE.
Maximum authorised draught 5 m.
VHF REPORTING
Vessels > 300 GRT and/or with draught  > 4 m shall report to
the ferry on VHF CH 11 or by phone on
+46 (0)771-656 565 not later than 15 minutes before passage.