ØSTERRENDEN (EASTERN CHANNEL) - EAST BRIDGE

Passage is only allowed for vessels with an air draught of less than 65,0
metres.
Vessels of 20 metres and above shall use the traffic lanes in the traffic
separation scheme. Vessels with an overall length not exceeding 20 metres
and sailing vessels shall as far as possible avoid using the traffic lanes
of the traffic separation scheme and instead use the adjacent connection
spans.
Before entering the traffic separation scheme the speed should be reduced
to maximum 20 knots.
Fishing is prohibited in the traffic lanes in the traffic separation scheme. 
