WIND FARM HORNS REV 2
Anchoring and any use of gear towed on the bottom are prohibited within the submarine cable area which is established with a protection zone extending 200 metres around the wind farm and the transformer platform.
