POSITION REPORTING SYSTEM NAKSKOV FJORD
When the Reporting Points shown are being passed, a report 
must be given on VHF channel 12 (without address). The 
report must contain: The name of the vessel, direction 
(inward bound/outward bound), position, and draught. On 
departure from Nakskov Harbour, also berth number. An 
oncoming vessel must reply immediately so that the two 
vessels can arrange a safe passage.
