
WIND FARM HORNS REV 1
Anchoring and any use of gear towed on the bottom are prohibited within 
the submarine cable area which is established with a protection zone 
extending 200 metres around the wind farm and the transformer platform.

Recording stations marked by yellow
buoys (Fl(5)Y.20s) may be established in the wind farm.