TRAFFIC SEPARATION SCHEME AND
DW ROUTE AT HATTER BARN
The traffic separation scheme at Hatter Barn
shall be used in accordance with Rule 10 of
the International Regulations for Preventing
Collisions at Sea.
The traffic lanes in the traffic separation
scheme have a minimum depth of 15 metres
and shall be used by ships with a draught
not exceeding 13 metres.
The 19 metres DW Route between Hatterrev
and Hatter Barn is intended for use only by
ships with a draught of more than 13 metres.
