TSS Terschelling - German Bight

The following container vessels are at risk of losing containers and touching the seabed 
during heavy weather and high waves from a west-northwest to north-easterly direction:

- Container vessels of 100-200m in length.
With a wave height of more than 3.0m. Masters must take appropriate measures and 
alter course if necessary to avoid broaching and coming abeam to the waves.

- Container vessels of more than  200m in length. 
With a wave height over 4.0m. Masters must take appropriate measures and 
alter course if necessary to avoid broaching and coming abeam to the waves.
Masters are recommended to follow an alternative route 
via TSS East Friesland.