
VESSEL TRAFFIC SERVICE IN FEMERN BELT - VTS FEMERN BELT
It is recommended that ships intending to pass the VTS area report on VHF channel 68. The call shall be made when the ship passes the reporting lines shown.
The report from the ship to the VTS should contain the following information: Ship's name and/or call sign, ship's draught, destination and planned route and any other safety related information deemed necessary.
Shipping is requested to be on standby on VHF channels 68 and 16 in the VTS area.
Information about activities and the location of the work areas will be available via Danish Chart Corrections (www.gst.dk), Danish Notices to Mariners (www.sfs.dk) and NAVTEX.
