MAGNETIC COMPASS DEFLECTIONS	
Magnetic compass deflections of up to 70° can occur near the
highvoltage direct current cable. Switch off your magnetic
compass autopilot before you sail across the cable. Whenever
possible, do so quickly and at a right angle.
