GENERAL CALL

Vessels of 300 GT or more and vessels, including tows, 
with a length of 45 meters or more should make a 
General call in English on VHF Ch 16 fifteen (15) minutes 
before passing the reporting point and when departing from 
a quay or anchorage. 

Following information should be stated:  
A. ALL SHIPS call and VHF Ch
B. Ship type and ships name
C. Name and location of reporting point or place of departure
D. Intended route
E. Destination

Smaller vessels fitted with a VHF should report if the 
circumstances so admit.