GENERAL CALL
A General call on VHF Ch 16 should be made by all inbound vessels 
or tows of 300 GT or 45 meters in length when passing the 
reporting points 1 or 2, when departing from a quay in Kalmar 
or an anchorage in the area between the reporting points.  

Smaller vessels should report if the circumstances admits.

Following information should be stated:  
A. All ships call and VHF Ch  
B. Ship type and ships name  
C. Name and location of reporting point or place of departure  
D. Intended route  
E. Destination  

AREA
Waters between following reporting points:
Nr 1 Hagbygrundet	56-32,0N	16-18,0E
Nr 2 Sillåsen		56-47,0N	16-30,5E
