MÄLAREN WATERWAY
The waterway between Södertälje and Västerås/Köping:
Maximum draught  ...................  6,8 m
Vertical clearance  ...................  34,0 m
8,4 m depth contour in vicinity of the waterway