GAS PIPELINE
Anchoring and any use of gear towed on the bottom is prohibited
in the protection zone which extends 200 metres on each side of 
the pipeline. Gas from a damaged pipeline could cause an explosion, 
loss of a vessel's buoyancy or other serious hazard.
