DEPTHS IN THE DREDGED CHANNEL AND THE PORT
Charted depths in the dredged channel and the port are given at Mean Low 
Water Springs (MLWS). The depth at Mean Low Water Springs (MLWS) in the 
dredged channel is 10.30 m in the leading line decreasing to 9.80 m at the 
borders. At Lowest Astronomical Tide (LAT) the depths in the dredged 
channel and the port are 0.45 m lesser.
